
\chapter{Pinout}

The \chip\ is packaged in a 68-pin PLCC with the following pinout


\figonecol[!b]{cam-chip-pinout}{\ttbox{fig/cam-chip-pinout.tt}}{External \bus\ host cable.}

\flushpage
