% -*- Mode:Text -*- 
% tt 12-27-94				DATA SHEETS
\documentclass{book}
\usepackage{epsfig}

 \title{Data Sheets}
 \input ../stepx                % format and terms of STEP context
 \input manx                    % specific terms of this manual


%----------------------------------------------------------------
% for each device, add a file named +nnn.tex, containing \dodevice
% for each maker, add a file named +nnn.tex containing \flushpage

\includeonly{_cover,_pref,_toc,+national,+AC08}
%\includeonly{_cover,_pref,_toc}

\begin{document}

\frontmatter
\include{_cover}
\twocolumn
\include{_pref} 
\include{_toc}

\mainmatter
\onecolumn
\pagestyle{myheadings}

% \Appendix{Components (by manufacturer and part number)}

 \maker{AMP}{amp}
	\includedevice{Contact Arrangements}{AMP12}{}{2}
%	\includedevice{Panel Cutout Specs}{AMP10}{}{2}
	\includedevice{Panel Cutout Specs}{AMP10}{}{1}
	\includedevice{205817-3}{AMP22}{VGA screwlock set}{1}
	\includedevice{748565-1}{AMP20}{VGA panel receptacle}{1}
	\includedevice{748610-4}{AMP21}{VGA female pins}{1}
	\includedevice{749075-5}{AMP1}{right-angle header}{1}
	\includedevice{749076-5}{AMP3}{right-angle header}{1}
	\includedevice{749084-5}{AMP5}{right-angle plug}{1}
	\includedevice{749086-1/087-1/087-2}{AMP11}{screwlock kits}{1}
	\includedevice{749611-5}{AMP7}{panel receptacle}{1}
	\includedevice{749621-5}{AMP2}{cable plug}{1}
	\includedevice{749649-5}{AMP4}{right-angle header}{1}
	\includedevice{749656-5}{AMP8}{panel receptacle}{1}
	\includedevice{749699-5}{AMP6}{cable receptacle}{1}
	\includedevice{749877-5}{AMP9}{panel receptacle}{1}
	\includedevice{821977-1}{AMP13}{32-pin PLCC socket}{3}
 \maker{Atmel}{atmel}
	\includedevice{AT27C256R}{AT27C256}{256K EPROM}{8}
 \maker{Augat}{augat}
	\includedevice{PCS-020/028SMU-11}{augat1}{20/28-pin PLCC sockets}{2}
 \maker{Berg}{berg}
	\includedevice{65043-032}{boxhse}{mini-latch housing}{2}
	\includedevice{47748-000}{boxpin}{crimp receptacle}{3}
	\includedevice{66245-250}{quickie}{backplane receptacle}{2}
	\includedevice{66247-008}{quickie-shroud}{backplane shroud}{2}
 \maker{Brooktree}{brooktree}
	\includedevice{Bt478}{Bt478}{color palette RAMDAC}{23}
	\includedevice{Bt858}{Bt858}{RGB-to-video encoder}{59}
 \maker{Data Delay Devices}{ddd}
	\includedevice{DDU-7F-10}{DDU-7F-10}{digital delay unit}{1}
 \maker{Fujitsu}{fuji}
	\includedevice{FCN-234P096-G/0}{sbus}{SBus connector}{2}
 \maker{Hirose}{hirose}
	\includedevice{HR10A-10R-12S}{hirose1}{circular panel mount recept.}{2}
 \maker{IDT}{idt}
	\includedevice{IDT72211}{IDT72211}{FIFO}{18}
 \maker{Lattice Semiconductor}{lattice}
	\includedevice{GAL16V8B}{16v8}{programmable logic device}{19}
	\includedevice{GAL22V10B}{22v10}{programmable logic device}{20}
 \maker{LZRelectronics}{LZRelectronics}
	\includedevice{LZR-MDJCP4}{LZR-MDJCP4}{mini-DIN panel mount recept.}{1}
 \maker{Maxim}{maxim}
	\includedevice{MAX698}{MAX698}{power-on reset}{3}
 \maker{Molex}{molex}
	\includedevice{03-06-1023/2023}{molex1}{recept.~/plug shell}{1}
	\includedevice{02-06-1103/2103}{molex2}{female/male pin}{1}
 \maker{Motorola}{motorola}
	\includedevice{MC10H645}{MC10H645}{clock buffer}{4}
	\includedevice{MC88915}{MC88915}{phase-locked loop}{13}
 \maker{MUPAC}{mupac}
	\includedevice{3351050-02-PKG}{eject}{inserter/ejector}{1}
 \maker{National Semiconductor}{national}
	\includedevice{BAV99}{BAV99}{silicon diode pair}{1}
	\includedevice{LM385-1.2}{LM385}{voltage reference}{2}
	\includedevice{74AC08}{AC08}{quad AND gate}{4}
	\includedevice{74AC377}{AC377}{octal D flip-flop}{6}
	\includedevice{74ACQ244}{ACQ244}{octal buffer}{5}
	\includedevice{74ACQ245}{ACQ245}{octal transceiver}{5}
	\includedevice{74ACQ374}{ACQ374}{octal D flip-flop}{4}
 \maker{OKI Semiconductor}{oki}
	\includedevice{MSM514402}{MSM514402}{4M DRAM}{14}
 \maker{Texas Instruments}{ti}
	\includedevice{TIBPAL16L8/16R4}{PAL16L8}{programmable array logic}{16}
 \maker{Toshiba}{toshiba}
	\includedevice{TC5117400}{TC5117400}{16M DRAM}{20}
	\includedevice{TC514400}{TC514400}{4M DRAM}{19}
	\includedevice{TC524256}{TC524256}{1M video RAM}{37}
	\includedevice{TC55464}{TC55464}{256K SRAM}{9}
 \maker{TRW}{trw}
	\includedevice{TMC1175}{TMC1175}{A/D converter}{12}

 \makeatletter
 \renewcommand{\@oddhead}{}
 \renewcommand{\@evenhead}{}
 \makeatother
 \null

\end{document}

% 373 pages
